	Front/Back Door Acceleration (100%/sē)

[const]
fdoor_acc
1.3

[const]
bdoor_acc
1.3

[const]
fdoor_acc2L
2.3

[const]
fdoor_acc2R
2.3

[const]
fdoor_acc3L
2.3

[const]
fdoor_acc3R
2.3

[const]
fdoor_acc4L
2.3

[const]
fdoor_acc4R
2.3

	Door Acceleration Variation (100%/sē)

[const]
door_acc_var
0.0

[const]
door_acc_var2L
0.0

[const]
door_acc_var2R
0.0

[const]
door_acc_var3L
0.0

[const]
door_acc_var3R
0.0

[const]
door_acc_var4L
0.0

[const]
door_acc_var4R
0.0

	Front/Back Door Max Speed (100%/s)

[const]
fdoor_maxspeed
2

[const]
fdoor_maxspeed2L
2

[const]
fdoor_maxspeed2R
2

[const]
fdoor_maxspeed3L
2

[const]
fdoor_maxspeed3R
2

[const]
fdoor_maxspeed4L
2

[const]
fdoor_maxspeed4R
2

[const]
bdoor_maxspeed
2

[const]
door_maxspeed_var
2

[const]
door_maxspeed_var2L
2

[const]
door_maxspeed_var2R
2

[const]
door_maxspeed_var3L
2

[const]
door_maxspeed_var3R
2

[const]
door_maxspeed_var4L
2

[const]
door_maxspeed_var4R
2

	Door Stop Reflexion Coefficient

[const]
door_refl
0.1

[const]
door_refl2L
0.1

[const]
door_refl2R
0.1

[const]
door_refl3L
0.1

[const]
door_refl3R
0.1

[const]
door_refl4L
0.1

[const]
door_refl4R
0.1

	Automatic Back Door Time

[const]
doorAftOpenTime
3

	Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
2

[const]
door_druckluft
1

[const]
door_needs_stopbrake
0

[const]
electric_doors
0

[newcurve]
door_0_opn_speed

[pnt]
0
0.2

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
0.85
0.01

[pnt]
0.95
0.01

[pnt]
1
0.4

[newcurve]
door_0_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.07

[pnt]
0.25
0.07

[pnt]
0.3
0.75

[pnt]
1
0.9

[newcurve]
door_1_opn_speed

[pnt]
0
0.42

[pnt]
0.2
0.72

[pnt]
0.8
0.67

[pnt]
0.85
0.07

[pnt]
0.95
0.07

[pnt]
1
0.4

[newcurve]
door_1_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.07

[pnt]
0.2
0.07

[pnt]
0.3
0.8

[pnt]
1
0.9




[newcurve]
door_2L_opn_speed

[pnt]
0
0.2

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
0.85
0.01

[pnt]
0.95
0.01

[pnt]
1
0.4

[newcurve]
door_2L_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.07

[pnt]
0.25
0.07

[pnt]
0.3
0.8

[pnt]
1
0.9



[newcurve]
door_2R_opn_speed

[pnt]
0
0.2

[pnt]
0.2
0.6

[pnt]
0.8
0.6

[pnt]
0.85
0.05

[pnt]
0.95
0.05

[pnt]
1
0.5

[newcurve]
door_2R_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.05

[pnt]
0.25
0.05

[pnt]
0.3
0.7

[pnt]
1
0.8



[newcurve]
door_3L_opn_speed

[pnt]
0
0.32

[pnt]
0.2
0.82

[pnt]
0.8
0.67

[pnt]
0.85
0.01

[pnt]
0.95
0.01

[pnt]
1
0.4

[newcurve]
door_3L_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.07

[pnt]
0.25
0.07

[pnt]
0.3
0.8

[pnt]
1
0.9



[newcurve]
door_3R_opn_speed

[pnt]
0
0.33

[pnt]
0.2
0.73

[pnt]
0.8
0.67

[pnt]
0.85
0.05

[pnt]
0.95
0.05

[pnt]
1
0.5

[newcurve]
door_3R_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.05

[pnt]
0.25
0.05

[pnt]
0.3
0.7

[pnt]
1
0.8

[newcurve]
door_4L_opn_speed

[pnt]
0
0.32

[pnt]
0.2
0.82

[pnt]
0.8
0.67

[pnt]
0.85
0.01

[pnt]
0.95
0.01

[pnt]
1
0.4

[newcurve]
door_4L_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.07

[pnt]
0.25
0.07

[pnt]
0.3
0.8

[pnt]
1
0.9



[newcurve]
door_4R_opn_speed

[pnt]
0
0.33

[pnt]
0.2
0.73

[pnt]
0.8
0.67

[pnt]
0.85
0.05

[pnt]
0.95
0.05

[pnt]
1
0.5

[newcurve]
door_4R_cls_speed

[pnt]
0
0.5

[pnt]
0.1
0.05

[pnt]
0.25
0.05

[pnt]
0.3
0.7

[pnt]
1
0.8